# do not edit this file, it will be overwritten on update

ACTION=="remove", GOTO="sensor_end"

# device matching the sensor's label, name and the machine's DMI data for IIO devices
SUBSYSTEM=="iio", KERNEL=="iio*", SUBSYSTEMS=="usb|i2c|platform", ATTR{label}!="", \
  IMPORT{builtin}="hwdb 'sensor:$attr{label}:modalias:$attr{modalias}:$attr{[dmi/id]modalias}'", \
  GOTO="sensor_end"

# Before Linux v6.0, cros-ec-accel used a non-standard 'location' sysfs file
SUBSYSTEM=="iio", KERNEL=="iio*", SUBSYSTEMS=="platform", \
  ATTR{name}=="cros-ec-accel|cros-ec-accel-legacy", ATTR{location}=="base", \
  IMPORT{builtin}="hwdb 'sensor:accel-base:modalias:$attr{modalias}:$attr{[dmi/id]modalias}'", \
  GOTO="sensor_end"

SUBSYSTEM=="iio", KERNEL=="iio*", SUBSYSTEMS=="platform", \
  ATTR{name}=="cros-ec-accel|cros-ec-accel-legacy", ATTR{location}=="lid", \
  IMPORT{builtin}="hwdb 'sensor:accel-display:modalias:$attr{modalias}:$attr{[dmi/id]modalias}'", \
  GOTO="sensor_end"

# device matching the sensor's name and the machine's DMI data for IIO devices
SUBSYSTEM=="iio", KERNEL=="iio*", SUBSYSTEMS=="usb|i2c|platform", \
  IMPORT{builtin}="hwdb 'sensor:modalias:$attr{modalias}:$attr{[dmi/id]modalias}'", \
  GOTO="sensor_end"

SUBSYSTEM=="input", ENV{ID_INPUT_ACCELEROMETER}=="1", SUBSYSTEMS=="acpi", \
  IMPORT{builtin}="hwdb 'sensor:modalias:acpi:$attr{hid}:$attr{[dmi/id]modalias}'", \
  GOTO="sensor_end"

SUBSYSTEM=="input", ENV{ID_INPUT_ACCELEROMETER}=="1", SUBSYSTEMS=="platform", \
  IMPORT{builtin}="hwdb 'sensor:modalias:platform:$id:$attr{[dmi/id]modalias}'", \
  GOTO="sensor_end"

LABEL="sensor_end"
