# do not edit this file, it will be overwritten on update

ACTION=="remove", GOTO="net_dhcp_end"
SUBSYSTEM!="net", GOTO="net_dhcp_end"

# Network interfaces requiring DHCPOFFER messages to be broadcast
# must set ID_NET_DHCP_BROADCAST to "1". This property will be
# checked by the networkd DHCP4 client to set the DHCP option

# s390 ccwgroup interfaces in layer3 mode need broadcast DHCPOFFER
# using the link driver to detect this condition
ENV{ID_NET_DRIVER}=="qeth_l3", ENV{ID_NET_DHCP_BROADCAST}="1"

LABEL="net_dhcp_end"
