# do not edit this file, it will be overwritten on update

ACTION=="remove", GOTO="serial_end"
SUBSYSTEM!="tty", GOTO="serial_end"

SUBSYSTEMS=="usb", IMPORT{builtin}="usb_id", IMPORT{builtin}="hwdb --subsystem=usb"
SUBSYSTEMS=="pci", ENV{ID_BUS}=="", ENV{ID_BUS}="pci", \
  ENV{ID_VENDOR_ID}="$attr{vendor}", ENV{ID_MODEL_ID}="$attr{device}", \
  IMPORT{builtin}="hwdb --subsystem=pci"

# /dev/serial/by-path/, /dev/serial/by-id/ for USB devices
KERNEL!="ttyUSB[0-9]*|ttyACM[0-9]*", GOTO="serial_end"

SUBSYSTEMS=="usb-serial", ENV{.ID_PORT}="$attr{port_number}"

IMPORT{builtin}="path_id"
ENV{ID_PATH}=="?*",                   ENV{.ID_PORT}=="",   SYMLINK+="serial/by-path/$env{ID_PATH}"
ENV{ID_PATH_WITH_USB_REVISION}=="?*", ENV{.ID_PORT}=="",   SYMLINK+="serial/by-path/$env{ID_PATH_WITH_USB_REVISION}"
ENV{ID_PATH}=="?*",                   ENV{.ID_PORT}=="?*", SYMLINK+="serial/by-path/$env{ID_PATH}-port$env{.ID_PORT}"
ENV{ID_PATH_WITH_USB_REVISION}=="?*", ENV{.ID_PORT}=="?*", SYMLINK+="serial/by-path/$env{ID_PATH_WITH_USB_REVISION}-port$env{.ID_PORT}"

ENV{ID_BUS}=="", GOTO="serial_end"
ENV{ID_SERIAL}=="", GOTO="serial_end"
ENV{ID_USB_INTERFACE_NUM}=="", GOTO="serial_end"
ENV{.ID_PORT}=="", SYMLINK+="serial/by-id/$env{ID_BUS}-$env{ID_SERIAL}-if$env{ID_USB_INTERFACE_NUM}"
ENV{.ID_PORT}=="?*", SYMLINK+="serial/by-id/$env{ID_BUS}-$env{ID_SERIAL}-if$env{ID_USB_INTERFACE_NUM}-port$env{.ID_PORT}"

LABEL="serial_end"
