# This file is part of systemd.
#
# Data imported from: http://pci-ids.ucw.cz/v2.2/pci.ids

pci:v*d*sv*sd*bc00*
 ID_PCI_CLASS_FROM_DATABASE=Unclassified device

pci:v*d*sv*sd*bc00sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=Non-VGA unclassified device

pci:v*d*sv*sd*bc00sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=VGA compatible unclassified device

pci:v*d*sv*sd*bc00sc05*
 ID_PCI_SUBCLASS_FROM_DATABASE=Image coprocessor

pci:v*d*sv*sd*bc01*
 ID_PCI_CLASS_FROM_DATABASE=Mass storage controller

pci:v*d*sv*sd*bc01sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=SCSI storage controller

pci:v*d*sv*sd*bc01sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=IDE interface

pci:v*d*sv*sd*bc01sc01i00*
 ID_PCI_INTERFACE_FROM_DATABASE=ISA Compatibility mode-only controller

pci:v*d*sv*sd*bc01sc01i05*
 ID_PCI_INTERFACE_FROM_DATABASE=PCI native mode-only controller

pci:v*d*sv*sd*bc01sc01i0A*
 ID_PCI_INTERFACE_FROM_DATABASE=ISA Compatibility mode controller, supports both channels switched to PCI native mode

pci:v*d*sv*sd*bc01sc01i0F*
 ID_PCI_INTERFACE_FROM_DATABASE=PCI native mode controller, supports both channels switched to ISA compatibility mode

pci:v*d*sv*sd*bc01sc01i80*
 ID_PCI_INTERFACE_FROM_DATABASE=ISA Compatibility mode-only controller, supports bus mastering

pci:v*d*sv*sd*bc01sc01i85*
 ID_PCI_INTERFACE_FROM_DATABASE=PCI native mode-only controller, supports bus mastering

pci:v*d*sv*sd*bc01sc01i8A*
 ID_PCI_INTERFACE_FROM_DATABASE=ISA Compatibility mode controller, supports both channels switched to PCI native mode, supports bus mastering

pci:v*d*sv*sd*bc01sc01i8F*
 ID_PCI_INTERFACE_FROM_DATABASE=PCI native mode controller, supports both channels switched to ISA compatibility mode, supports bus mastering

pci:v*d*sv*sd*bc01sc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=Floppy disk controller

pci:v*d*sv*sd*bc01sc03*
 ID_PCI_SUBCLASS_FROM_DATABASE=IPI bus controller

pci:v*d*sv*sd*bc01sc04*
 ID_PCI_SUBCLASS_FROM_DATABASE=RAID bus controller

pci:v*d*sv*sd*bc01sc05*
 ID_PCI_SUBCLASS_FROM_DATABASE=ATA controller

pci:v*d*sv*sd*bc01sc05i20*
 ID_PCI_INTERFACE_FROM_DATABASE=ADMA single stepping

pci:v*d*sv*sd*bc01sc05i30*
 ID_PCI_INTERFACE_FROM_DATABASE=ADMA continuous operation

pci:v*d*sv*sd*bc01sc06*
 ID_PCI_SUBCLASS_FROM_DATABASE=SATA controller

pci:v*d*sv*sd*bc01sc06i00*
 ID_PCI_INTERFACE_FROM_DATABASE=Vendor specific

pci:v*d*sv*sd*bc01sc06i01*
 ID_PCI_INTERFACE_FROM_DATABASE=AHCI 1.0

pci:v*d*sv*sd*bc01sc06i02*
 ID_PCI_INTERFACE_FROM_DATABASE=Serial Storage Bus

pci:v*d*sv*sd*bc01sc07*
 ID_PCI_SUBCLASS_FROM_DATABASE=Serial Attached SCSI controller

pci:v*d*sv*sd*bc01sc07i01*
 ID_PCI_INTERFACE_FROM_DATABASE=Serial Storage Bus

pci:v*d*sv*sd*bc01sc08*
 ID_PCI_SUBCLASS_FROM_DATABASE=Non-Volatile memory controller

pci:v*d*sv*sd*bc01sc08i01*
 ID_PCI_INTERFACE_FROM_DATABASE=NVMHCI

pci:v*d*sv*sd*bc01sc08i02*
 ID_PCI_INTERFACE_FROM_DATABASE=NVM Express

pci:v*d*sv*sd*bc01sc09*
 ID_PCI_SUBCLASS_FROM_DATABASE=Universal Flash Storage controller

pci:v*d*sv*sd*bc01sc09i00*
 ID_PCI_INTERFACE_FROM_DATABASE=Vendor specific

pci:v*d*sv*sd*bc01sc09i01*
 ID_PCI_INTERFACE_FROM_DATABASE=UFSHCI

pci:v*d*sv*sd*bc01sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Mass storage controller

pci:v*d*sv*sd*bc02*
 ID_PCI_CLASS_FROM_DATABASE=Network controller

pci:v*d*sv*sd*bc02sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=Ethernet controller

pci:v*d*sv*sd*bc02sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=Token ring network controller

pci:v*d*sv*sd*bc02sc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=FDDI network controller

pci:v*d*sv*sd*bc02sc03*
 ID_PCI_SUBCLASS_FROM_DATABASE=ATM network controller

pci:v*d*sv*sd*bc02sc04*
 ID_PCI_SUBCLASS_FROM_DATABASE=ISDN controller

pci:v*d*sv*sd*bc02sc05*
 ID_PCI_SUBCLASS_FROM_DATABASE=WorldFip controller

pci:v*d*sv*sd*bc02sc06*
 ID_PCI_SUBCLASS_FROM_DATABASE=PICMG controller

pci:v*d*sv*sd*bc02sc07*
 ID_PCI_SUBCLASS_FROM_DATABASE=Infiniband controller

pci:v*d*sv*sd*bc02sc08*
 ID_PCI_SUBCLASS_FROM_DATABASE=Fabric controller

pci:v*d*sv*sd*bc02sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Network controller

pci:v*d*sv*sd*bc03*
 ID_PCI_CLASS_FROM_DATABASE=Display controller

pci:v*d*sv*sd*bc03sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=VGA compatible controller

pci:v*d*sv*sd*bc03sc00i00*
 ID_PCI_INTERFACE_FROM_DATABASE=VGA controller

pci:v*d*sv*sd*bc03sc00i01*
 ID_PCI_INTERFACE_FROM_DATABASE=8514 controller

pci:v*d*sv*sd*bc03sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=XGA compatible controller

pci:v*d*sv*sd*bc03sc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=3D controller

pci:v*d*sv*sd*bc03sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Display controller

pci:v*d*sv*sd*bc04*
 ID_PCI_CLASS_FROM_DATABASE=Multimedia controller

pci:v*d*sv*sd*bc04sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=Multimedia video controller

pci:v*d*sv*sd*bc04sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=Multimedia audio controller

pci:v*d*sv*sd*bc04sc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=Computer telephony device

pci:v*d*sv*sd*bc04sc03*
 ID_PCI_SUBCLASS_FROM_DATABASE=Audio device

pci:v*d*sv*sd*bc04sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Multimedia controller

pci:v*d*sv*sd*bc05*
 ID_PCI_CLASS_FROM_DATABASE=Memory controller

pci:v*d*sv*sd*bc05sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=RAM memory

pci:v*d*sv*sd*bc05sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=FLASH memory

pci:v*d*sv*sd*bc05sc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=CXL

pci:v*d*sv*sd*bc05sc02i00*
 ID_PCI_INTERFACE_FROM_DATABASE=CXL Memory Device - vendor specific

pci:v*d*sv*sd*bc05sc02i10*
 ID_PCI_INTERFACE_FROM_DATABASE=CXL Memory Device (CXL 2.x)

pci:v*d*sv*sd*bc05sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Memory controller

pci:v*d*sv*sd*bc06*
 ID_PCI_CLASS_FROM_DATABASE=Bridge

pci:v*d*sv*sd*bc06sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=Host bridge

pci:v*d*sv*sd*bc06sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=ISA bridge

pci:v*d*sv*sd*bc06sc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=EISA bridge

pci:v*d*sv*sd*bc06sc03*
 ID_PCI_SUBCLASS_FROM_DATABASE=MicroChannel bridge

pci:v*d*sv*sd*bc06sc04*
 ID_PCI_SUBCLASS_FROM_DATABASE=PCI bridge

pci:v*d*sv*sd*bc06sc04i00*
 ID_PCI_INTERFACE_FROM_DATABASE=Normal decode

pci:v*d*sv*sd*bc06sc04i01*
 ID_PCI_INTERFACE_FROM_DATABASE=Subtractive decode

pci:v*d*sv*sd*bc06sc05*
 ID_PCI_SUBCLASS_FROM_DATABASE=PCMCIA bridge

pci:v*d*sv*sd*bc06sc06*
 ID_PCI_SUBCLASS_FROM_DATABASE=NuBus bridge

pci:v*d*sv*sd*bc06sc07*
 ID_PCI_SUBCLASS_FROM_DATABASE=CardBus bridge

pci:v*d*sv*sd*bc06sc08*
 ID_PCI_SUBCLASS_FROM_DATABASE=RACEway bridge

pci:v*d*sv*sd*bc06sc08i00*
 ID_PCI_INTERFACE_FROM_DATABASE=Transparent mode

pci:v*d*sv*sd*bc06sc08i01*
 ID_PCI_INTERFACE_FROM_DATABASE=Endpoint mode

pci:v*d*sv*sd*bc06sc09*
 ID_PCI_SUBCLASS_FROM_DATABASE=Semi-transparent PCI-to-PCI bridge

pci:v*d*sv*sd*bc06sc09i40*
 ID_PCI_INTERFACE_FROM_DATABASE=Primary bus towards host CPU

pci:v*d*sv*sd*bc06sc09i80*
 ID_PCI_INTERFACE_FROM_DATABASE=Secondary bus towards host CPU

pci:v*d*sv*sd*bc06sc0A*
 ID_PCI_SUBCLASS_FROM_DATABASE=InfiniBand to PCI host bridge

pci:v*d*sv*sd*bc06sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Bridge

pci:v*d*sv*sd*bc07*
 ID_PCI_CLASS_FROM_DATABASE=Communication controller

pci:v*d*sv*sd*bc07sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=Serial controller

pci:v*d*sv*sd*bc07sc00i00*
 ID_PCI_INTERFACE_FROM_DATABASE=8250

pci:v*d*sv*sd*bc07sc00i01*
 ID_PCI_INTERFACE_FROM_DATABASE=16450

pci:v*d*sv*sd*bc07sc00i02*
 ID_PCI_INTERFACE_FROM_DATABASE=16550

pci:v*d*sv*sd*bc07sc00i03*
 ID_PCI_INTERFACE_FROM_DATABASE=16650

pci:v*d*sv*sd*bc07sc00i04*
 ID_PCI_INTERFACE_FROM_DATABASE=16750

pci:v*d*sv*sd*bc07sc00i05*
 ID_PCI_INTERFACE_FROM_DATABASE=16850

pci:v*d*sv*sd*bc07sc00i06*
 ID_PCI_INTERFACE_FROM_DATABASE=16950

pci:v*d*sv*sd*bc07sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=Parallel controller

pci:v*d*sv*sd*bc07sc01i00*
 ID_PCI_INTERFACE_FROM_DATABASE=SPP

pci:v*d*sv*sd*bc07sc01i01*
 ID_PCI_INTERFACE_FROM_DATABASE=BiDir

pci:v*d*sv*sd*bc07sc01i02*
 ID_PCI_INTERFACE_FROM_DATABASE=ECP

pci:v*d*sv*sd*bc07sc01i03*
 ID_PCI_INTERFACE_FROM_DATABASE=IEEE1284

pci:v*d*sv*sd*bc07sc01iFE*
 ID_PCI_INTERFACE_FROM_DATABASE=IEEE1284 Target

pci:v*d*sv*sd*bc07sc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=Multiport serial controller

pci:v*d*sv*sd*bc07sc03*
 ID_PCI_SUBCLASS_FROM_DATABASE=Modem

pci:v*d*sv*sd*bc07sc03i00*
 ID_PCI_INTERFACE_FROM_DATABASE=Generic

pci:v*d*sv*sd*bc07sc03i01*
 ID_PCI_INTERFACE_FROM_DATABASE=Hayes/16450

pci:v*d*sv*sd*bc07sc03i02*
 ID_PCI_INTERFACE_FROM_DATABASE=Hayes/16550

pci:v*d*sv*sd*bc07sc03i03*
 ID_PCI_INTERFACE_FROM_DATABASE=Hayes/16650

pci:v*d*sv*sd*bc07sc03i04*
 ID_PCI_INTERFACE_FROM_DATABASE=Hayes/16750

pci:v*d*sv*sd*bc07sc04*
 ID_PCI_SUBCLASS_FROM_DATABASE=GPIB controller

pci:v*d*sv*sd*bc07sc05*
 ID_PCI_SUBCLASS_FROM_DATABASE=Smard Card controller

pci:v*d*sv*sd*bc07sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Communication controller

pci:v*d*sv*sd*bc08*
 ID_PCI_CLASS_FROM_DATABASE=Generic system peripheral

pci:v*d*sv*sd*bc08sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=PIC

pci:v*d*sv*sd*bc08sc00i00*
 ID_PCI_INTERFACE_FROM_DATABASE=8259

pci:v*d*sv*sd*bc08sc00i01*
 ID_PCI_INTERFACE_FROM_DATABASE=ISA PIC

pci:v*d*sv*sd*bc08sc00i02*
 ID_PCI_INTERFACE_FROM_DATABASE=EISA PIC

pci:v*d*sv*sd*bc08sc00i10*
 ID_PCI_INTERFACE_FROM_DATABASE=IO-APIC

pci:v*d*sv*sd*bc08sc00i20*
 ID_PCI_INTERFACE_FROM_DATABASE=IO(X)-APIC

pci:v*d*sv*sd*bc08sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=DMA controller

pci:v*d*sv*sd*bc08sc01i00*
 ID_PCI_INTERFACE_FROM_DATABASE=8237

pci:v*d*sv*sd*bc08sc01i01*
 ID_PCI_INTERFACE_FROM_DATABASE=ISA DMA

pci:v*d*sv*sd*bc08sc01i02*
 ID_PCI_INTERFACE_FROM_DATABASE=EISA DMA

pci:v*d*sv*sd*bc08sc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=Timer

pci:v*d*sv*sd*bc08sc02i00*
 ID_PCI_INTERFACE_FROM_DATABASE=8254

pci:v*d*sv*sd*bc08sc02i01*
 ID_PCI_INTERFACE_FROM_DATABASE=ISA Timer

pci:v*d*sv*sd*bc08sc02i02*
 ID_PCI_INTERFACE_FROM_DATABASE=EISA Timers

pci:v*d*sv*sd*bc08sc02i03*
 ID_PCI_INTERFACE_FROM_DATABASE=HPET

pci:v*d*sv*sd*bc08sc03*
 ID_PCI_SUBCLASS_FROM_DATABASE=RTC

pci:v*d*sv*sd*bc08sc03i00*
 ID_PCI_INTERFACE_FROM_DATABASE=Generic

pci:v*d*sv*sd*bc08sc03i01*
 ID_PCI_INTERFACE_FROM_DATABASE=ISA RTC

pci:v*d*sv*sd*bc08sc04*
 ID_PCI_SUBCLASS_FROM_DATABASE=PCI Hot-plug controller

pci:v*d*sv*sd*bc08sc05*
 ID_PCI_SUBCLASS_FROM_DATABASE=SD Host controller

pci:v*d*sv*sd*bc08sc06*
 ID_PCI_SUBCLASS_FROM_DATABASE=IOMMU

pci:v*d*sv*sd*bc08sc07*
 ID_PCI_SUBCLASS_FROM_DATABASE=Root Complex Event Collector

pci:v*d*sv*sd*bc08sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=System peripheral

pci:v*d*sv*sd*bc08sc99*
 ID_PCI_SUBCLASS_FROM_DATABASE=Timing Card

pci:v*d*sv*sd*bc08sc99i01*
 ID_PCI_INTERFACE_FROM_DATABASE=TAP Timing Card

pci:v*d*sv*sd*bc09*
 ID_PCI_CLASS_FROM_DATABASE=Input device controller

pci:v*d*sv*sd*bc09sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=Keyboard controller

pci:v*d*sv*sd*bc09sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=Digitizer Pen

pci:v*d*sv*sd*bc09sc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=Mouse controller

pci:v*d*sv*sd*bc09sc03*
 ID_PCI_SUBCLASS_FROM_DATABASE=Scanner controller

pci:v*d*sv*sd*bc09sc04*
 ID_PCI_SUBCLASS_FROM_DATABASE=Gameport controller

pci:v*d*sv*sd*bc09sc04i00*
 ID_PCI_INTERFACE_FROM_DATABASE=Generic

pci:v*d*sv*sd*bc09sc04i10*
 ID_PCI_INTERFACE_FROM_DATABASE=Extended

pci:v*d*sv*sd*bc09sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Input device controller

pci:v*d*sv*sd*bc0A*
 ID_PCI_CLASS_FROM_DATABASE=Docking station

pci:v*d*sv*sd*bc0Asc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=Generic Docking Station

pci:v*d*sv*sd*bc0Asc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Docking Station

pci:v*d*sv*sd*bc0B*
 ID_PCI_CLASS_FROM_DATABASE=Processor

pci:v*d*sv*sd*bc0Bsc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=386

pci:v*d*sv*sd*bc0Bsc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=486

pci:v*d*sv*sd*bc0Bsc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=Pentium

pci:v*d*sv*sd*bc0Bsc10*
 ID_PCI_SUBCLASS_FROM_DATABASE=Alpha

pci:v*d*sv*sd*bc0Bsc20*
 ID_PCI_SUBCLASS_FROM_DATABASE=Power PC

pci:v*d*sv*sd*bc0Bsc30*
 ID_PCI_SUBCLASS_FROM_DATABASE=MIPS

pci:v*d*sv*sd*bc0Bsc40*
 ID_PCI_SUBCLASS_FROM_DATABASE=Co-processor

pci:v*d*sv*sd*bc0C*
 ID_PCI_CLASS_FROM_DATABASE=Serial bus controller

pci:v*d*sv*sd*bc0Csc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=FireWire (IEEE 1394)

pci:v*d*sv*sd*bc0Csc00i00*
 ID_PCI_INTERFACE_FROM_DATABASE=Generic

pci:v*d*sv*sd*bc0Csc00i10*
 ID_PCI_INTERFACE_FROM_DATABASE=OHCI

pci:v*d*sv*sd*bc0Csc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=ACCESS Bus

pci:v*d*sv*sd*bc0Csc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=SSA

pci:v*d*sv*sd*bc0Csc03*
 ID_PCI_SUBCLASS_FROM_DATABASE=USB controller

pci:v*d*sv*sd*bc0Csc03i00*
 ID_PCI_INTERFACE_FROM_DATABASE=UHCI

pci:v*d*sv*sd*bc0Csc03i10*
 ID_PCI_INTERFACE_FROM_DATABASE=OHCI

pci:v*d*sv*sd*bc0Csc03i20*
 ID_PCI_INTERFACE_FROM_DATABASE=EHCI

pci:v*d*sv*sd*bc0Csc03i30*
 ID_PCI_INTERFACE_FROM_DATABASE=XHCI

pci:v*d*sv*sd*bc0Csc03i40*
 ID_PCI_INTERFACE_FROM_DATABASE=USB4 Host Interface

pci:v*d*sv*sd*bc0Csc03i80*
 ID_PCI_INTERFACE_FROM_DATABASE=Unspecified

pci:v*d*sv*sd*bc0Csc03iFE*
 ID_PCI_INTERFACE_FROM_DATABASE=USB Device

pci:v*d*sv*sd*bc0Csc04*
 ID_PCI_SUBCLASS_FROM_DATABASE=Fibre Channel

pci:v*d*sv*sd*bc0Csc05*
 ID_PCI_SUBCLASS_FROM_DATABASE=SMBus

pci:v*d*sv*sd*bc0Csc06*
 ID_PCI_SUBCLASS_FROM_DATABASE=InfiniBand

pci:v*d*sv*sd*bc0Csc07*
 ID_PCI_SUBCLASS_FROM_DATABASE=IPMI Interface

pci:v*d*sv*sd*bc0Csc07i00*
 ID_PCI_INTERFACE_FROM_DATABASE=SMIC

pci:v*d*sv*sd*bc0Csc07i01*
 ID_PCI_INTERFACE_FROM_DATABASE=KCS

pci:v*d*sv*sd*bc0Csc07i02*
 ID_PCI_INTERFACE_FROM_DATABASE=BT (Block Transfer)

pci:v*d*sv*sd*bc0Csc08*
 ID_PCI_SUBCLASS_FROM_DATABASE=SERCOS interface

pci:v*d*sv*sd*bc0Csc09*
 ID_PCI_SUBCLASS_FROM_DATABASE=CANBUS

pci:v*d*sv*sd*bc0Csc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Serial bus controller

pci:v*d*sv*sd*bc0D*
 ID_PCI_CLASS_FROM_DATABASE=Wireless controller

pci:v*d*sv*sd*bc0Dsc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=IRDA controller

pci:v*d*sv*sd*bc0Dsc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=Consumer IR controller

pci:v*d*sv*sd*bc0Dsc10*
 ID_PCI_SUBCLASS_FROM_DATABASE=RF controller

pci:v*d*sv*sd*bc0Dsc11*
 ID_PCI_SUBCLASS_FROM_DATABASE=Bluetooth

pci:v*d*sv*sd*bc0Dsc12*
 ID_PCI_SUBCLASS_FROM_DATABASE=Broadband

pci:v*d*sv*sd*bc0Dsc20*
 ID_PCI_SUBCLASS_FROM_DATABASE=802.1a controller

pci:v*d*sv*sd*bc0Dsc21*
 ID_PCI_SUBCLASS_FROM_DATABASE=802.1b controller

pci:v*d*sv*sd*bc0Dsc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Wireless controller

pci:v*d*sv*sd*bc0E*
 ID_PCI_CLASS_FROM_DATABASE=Intelligent controller

pci:v*d*sv*sd*bc0Esc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=I2O

pci:v*d*sv*sd*bc0F*
 ID_PCI_CLASS_FROM_DATABASE=Satellite communications controller

pci:v*d*sv*sd*bc0Fsc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=Satellite TV controller

pci:v*d*sv*sd*bc0Fsc02*
 ID_PCI_SUBCLASS_FROM_DATABASE=Satellite audio communication controller

pci:v*d*sv*sd*bc0Fsc03*
 ID_PCI_SUBCLASS_FROM_DATABASE=Satellite voice communication controller

pci:v*d*sv*sd*bc0Fsc04*
 ID_PCI_SUBCLASS_FROM_DATABASE=Satellite data communication controller

pci:v*d*sv*sd*bc10*
 ID_PCI_CLASS_FROM_DATABASE=Encryption controller

pci:v*d*sv*sd*bc10sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=Network and computing encryption device

pci:v*d*sv*sd*bc10sc10*
 ID_PCI_SUBCLASS_FROM_DATABASE=Entertainment encryption device

pci:v*d*sv*sd*bc10sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Encryption controller

pci:v*d*sv*sd*bc11*
 ID_PCI_CLASS_FROM_DATABASE=Signal processing controller

pci:v*d*sv*sd*bc11sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=DPIO module

pci:v*d*sv*sd*bc11sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=Performance counters

pci:v*d*sv*sd*bc11sc10*
 ID_PCI_SUBCLASS_FROM_DATABASE=Communication synchronizer

pci:v*d*sv*sd*bc11sc20*
 ID_PCI_SUBCLASS_FROM_DATABASE=Signal processing management

pci:v*d*sv*sd*bc11sc80*
 ID_PCI_SUBCLASS_FROM_DATABASE=Signal processing controller

pci:v*d*sv*sd*bc12*
 ID_PCI_CLASS_FROM_DATABASE=Processing accelerators

pci:v*d*sv*sd*bc12sc00*
 ID_PCI_SUBCLASS_FROM_DATABASE=Processing accelerators

pci:v*d*sv*sd*bc12sc01*
 ID_PCI_SUBCLASS_FROM_DATABASE=SNIA Smart Data Accelerator Interface (SDXI) controller

pci:v*d*sv*sd*bc13*
 ID_PCI_CLASS_FROM_DATABASE=Non-Essential Instrumentation

pci:v*d*sv*sd*bc40*
 ID_PCI_CLASS_FROM_DATABASE=Coprocessor

pci:v*d*sv*sd*bcFF*
 ID_PCI_CLASS_FROM_DATABASE=Unassigned class
