# do not edit this file, it will be overwritten on update

ACTION!="add", GOTO="autosuspend_end"

# I2C rules
SUBSYSTEM=="i2c", ATTR{name}=="cyapa", \
  ATTR{power/control}="on", GOTO="autosuspend_end"

# Enable autosuspend if hwdb says so. Here we are relying on
# the hwdb import done earlier based on MODALIAS.
ENV{ID_AUTOSUSPEND}=="1", TEST=="power/control", \
  ATTR{power/control}="auto"

# Disable USB persist if hwdb says so.
ENV{ID_PERSIST}=="0", TEST=="power/persist", \
  ATTR{power/persist}="0"

# Set up an autosuspend delay if hwdb say so
ENV{ID_AUTOSUSPEND_DELAY_MS}!="", TEST=="power/control", \
  ATTR{power/autosuspend_delay_ms}="$env{ID_AUTOSUSPEND_DELAY_MS}"

LABEL="autosuspend_end"
