# This file is part of systemd.
#
# Database for software-defined radio devices that should be accessible to the
# seat owner.
#
# The lookup keys are $MODALIAS strings, see udev's hwdb builtin.
#
# To add local entries, create a new file
#   /etc/udev/hwdb.d/71-software-radio-local.hwdb
# and add your rules there. To load the new rules execute (as root):
#   systemd-hwdb update
#   udevadm trigger /dev/…
#
# If your changes are generally applicable, send them as a pull request to
#   https://github.com/systemd/systemd
# or create a bug report on https://github.com/systemd/systemd/issues and
# include your new rules, a description of the device, and the output of
#   udevadm info
# for the device.
#
# Allowed properties are:
#   ID_SOFTWARE_RADIO=0|1

##########################################
# Analog Devices
##########################################
# ADI pluto SDR
usb:v0456pB673*
 ID_SOFTWARE_RADIO=1
 ID_MM_DEVICE_IGNORE=1

# ADI pluto DFU
usb:v0456pB674*
 ID_SOFTWARE_RADIO=1

##########################################
# Ettus Research
##########################################
# USRP1
usb:vFFFEp0002*
 ID_SOFTWARE_RADIO=1

# B100
usb:v2500p0002*
 ID_SOFTWARE_RADIO=1

# B200
usb:v2500p0020*
usb:v2500p0021*
usb:v2500p0022*
usb:v3923p7813*
usb:v3923p7814*
 ID_SOFTWARE_RADIO=1

##########################################
# Nuand
##########################################
# bladeRF 1.x
usb:v2CF0p5246*
 ID_SOFTWARE_RADIO=1

# bladeRF 1.x (legacy)
usb:v1D50p6066*
 ID_SOFTWARE_RADIO=1

# bladeRF 2.0 micro
usb:v2CF0p5250*
 ID_SOFTWARE_RADIO=1

##########################################
# RTL-SDR
##########################################
# original RTL2832U vid/pid (hama nano, for example)
usb:v0BDAp2832*
 ID_SOFTWARE_RADIO=1

# RTL2832U OEM vid/pid, e.g. ezcap EzTV668 (E4000), Newsky TV28T (E4000/R820T) etc.
usb:v0BDAp2838*
 ID_SOFTWARE_RADIO=1

# DigitalNow Quad DVB-T PCI-E card (4x FC0012?)
usb:v0413p6680*
 ID_SOFTWARE_RADIO=1

# Leadtek WinFast DTV Dongle mini D (FC0012)
usb:v0413p6F0F*
 ID_SOFTWARE_RADIO=1

# Genius TVGo DVB-T03 USB dongle (Ver. B)
usb:v0458p707F*
 ID_SOFTWARE_RADIO=1

# Terratec Cinergy T Stick Black (rev 1) (FC0012)
usb:v0CCDp00A9*
 ID_SOFTWARE_RADIO=1

# Terratec NOXON rev 1 (FC0013)
usb:v0CCDp00B3*
 ID_SOFTWARE_RADIO=1

# Terratec Deutschlandradio DAB Stick (FC0013)
usb:v0CCDp00B4*
 ID_SOFTWARE_RADIO=1

# Terratec NOXON DAB Stick - Radio Energy (FC0013)
usb:v0CCDp00B5*
 ID_SOFTWARE_RADIO=1

# Terratec Media Broadcast DAB Stick (FC0013)
usb:v0CCDp00B7*
 ID_SOFTWARE_RADIO=1

# Terratec BR DAB Stick (FC0013)
usb:v0CCDp00B8*
 ID_SOFTWARE_RADIO=1

# Terratec WDR DAB Stick (FC0013)
usb:v0CCDp00B9*
 ID_SOFTWARE_RADIO=1

# Terratec MuellerVerlag DAB Stick (FC0013)
usb:v0CCDp00C0*
 ID_SOFTWARE_RADIO=1

# Terratec Fraunhofer DAB Stick (FC0013)
usb:v0CCDp00C6*
 ID_SOFTWARE_RADIO=1

# Terratec Cinergy T Stick RC (Rev.3) (E4000)
usb:v0CCDp00D3*
 ID_SOFTWARE_RADIO=1

# Terratec T Stick PLUS (E4000)
usb:v0CCDp00D7*
 ID_SOFTWARE_RADIO=1

# Terratec NOXON rev 2 (E4000)
usb:v0CCDp00E0*
 ID_SOFTWARE_RADIO=1

# PixelView PV-DT235U(RN) (FC0012)
usb:v1554p5020*
 ID_SOFTWARE_RADIO=1

# Astrometa DVB-T/DVB-T2 (R828D)
usb:v15F4p0131*
 ID_SOFTWARE_RADIO=1

# HanfTek DAB+FM+DVB-T
usb:v15F4p0133*
 ID_SOFTWARE_RADIO=1

# Compro Videomate U620F (E4000)
usb:v185Bp0620*
 ID_SOFTWARE_RADIO=1

# Compro Videomate U650F (E4000)
usb:v185Bp0650*
 ID_SOFTWARE_RADIO=1

# Compro Videomate U680F (E4000)
usb:v185Bp0680*
 ID_SOFTWARE_RADIO=1

# GIGABYTE GT-U7300 (FC0012)
usb:v1B80pD393*
 ID_SOFTWARE_RADIO=1

# DIKOM USB-DVBT HD
usb:v1B80pD394*
 ID_SOFTWARE_RADIO=1

# Peak 102569AGPK (FC0012)
usb:v1B80pD395*
 ID_SOFTWARE_RADIO=1

# KWorld KW-UB450-T USB DVB-T Pico TV (TUA9001)
usb:v1B80pD397*
 ID_SOFTWARE_RADIO=1

# Zaapa ZT-MINDVBZP (FC0012)
usb:v1B80pD398*
 ID_SOFTWARE_RADIO=1

# SVEON STV20 DVB-T USB & FM (FC0012)
usb:v1B80pD39D*
 ID_SOFTWARE_RADIO=1

# Twintech UT-40 (FC0013)
usb:v1B80pD3A4*
 ID_SOFTWARE_RADIO=1

# ASUS U3100MINI_PLUS_V2 (FC0013)
usb:v1B80pD3A8*
 ID_SOFTWARE_RADIO=1

# SVEON STV27 DVB-T USB & FM (FC0013)
usb:v1B80pD3AF*
 ID_SOFTWARE_RADIO=1

# SVEON STV21 DVB-T USB & FM
usb:v1B80pD3B0*
 ID_SOFTWARE_RADIO=1

# Dexatek DK DVB-T Dongle (Logilink VG0002A) (FC2580)
usb:v1D19p1101*
 ID_SOFTWARE_RADIO=1

# Dexatek DK DVB-T Dongle (MSI DigiVox mini II V3.0)
usb:v1D19p1102*
 ID_SOFTWARE_RADIO=1

# Dexatek DK 5217 DVB-T Dongle (FC2580)
usb:v1D19p1103*
 ID_SOFTWARE_RADIO=1

# MSI DigiVox Micro HD (FC2580)
usb:v1D19p1104*
 ID_SOFTWARE_RADIO=1

# Sweex DVB-T USB (FC0012)
usb:v1F4DpA803*
 ID_SOFTWARE_RADIO=1

# GTek T803 (FC0012)
usb:v1F4DpB803*
 ID_SOFTWARE_RADIO=1

# Lifeview LV5TDeluxe (FC0012)
usb:v1F4DpC803*
 ID_SOFTWARE_RADIO=1

# MyGica TD312 (FC0012)
usb:v1F4DpD286*
 ID_SOFTWARE_RADIO=1

# PROlectrix DV107669 (FC0012)
usb:v1F4DpD803*
 ID_SOFTWARE_RADIO=1
