# do not edit this file, it will be overwritten on update

ACTION!="add|change|move|bind", GOTO="mm_dell_port_types_end"

SUBSYSTEMS=="usb", ATTRS{idVendor}=="413c", GOTO="mm_dell_vendorcheck"
GOTO="mm_dell_port_types_end"

LABEL="mm_dell_vendorcheck"
SUBSYSTEMS=="usb", ATTRS{bInterfaceNumber}=="?*", ENV{.MM_USBIFNUM}="$attr{bInterfaceNumber}"

# Dell DW5821e (default 0x81d7, with esim support 0x81e0)
#  if 02: primary port
#  if 03: secondary port
#  if 04: raw NMEA port
#  if 05: diag/qcdm port
ATTRS{idVendor}=="413c", ATTRS{idProduct}=="81d7", ENV{.MM_USBIFNUM}=="02", SUBSYSTEM=="tty", ENV{ID_MM_PORT_TYPE_AT_PRIMARY}="1"
ATTRS{idVendor}=="413c", ATTRS{idProduct}=="81d7", ENV{.MM_USBIFNUM}=="03", SUBSYSTEM=="tty", ENV{ID_MM_PORT_TYPE_AT_SECONDARY}="1"
ATTRS{idVendor}=="413c", ATTRS{idProduct}=="81d7", ENV{.MM_USBIFNUM}=="04", SUBSYSTEM=="tty", ENV{ID_MM_PORT_TYPE_GPS}="1"
ATTRS{idVendor}=="413c", ATTRS{idProduct}=="81d7", ENV{.MM_USBIFNUM}=="05", SUBSYSTEM=="tty", ENV{ID_MM_PORT_TYPE_QCDM}="1"
ATTRS{idVendor}=="413c", ATTRS{idProduct}=="81e0", ENV{.MM_USBIFNUM}=="02", SUBSYSTEM=="tty", ENV{ID_MM_PORT_TYPE_AT_PRIMARY}="1"
ATTRS{idVendor}=="413c", ATTRS{idProduct}=="81e0", ENV{.MM_USBIFNUM}=="03", SUBSYSTEM=="tty", ENV{ID_MM_PORT_TYPE_AT_SECONDARY}="1"
ATTRS{idVendor}=="413c", ATTRS{idProduct}=="81e0", ENV{.MM_USBIFNUM}=="04", SUBSYSTEM=="tty", ENV{ID_MM_PORT_TYPE_GPS}="1"
ATTRS{idVendor}=="413c", ATTRS{idProduct}=="81e0", ENV{.MM_USBIFNUM}=="05", SUBSYSTEM=="tty", ENV{ID_MM_PORT_TYPE_QCDM}="1"

# Dell DW5820e
#  if 02: AT port
#  if 04: debug port (ignore)
#  if 06: AT port
ATTRS{idVendor}=="413c", ATTRS{idProduct}=="81d9", ENV{.MM_USBIFNUM}=="04", ENV{ID_MM_PORT_IGNORE}="1"

GOTO="mm_dell_port_types_end"
LABEL="mm_dell_port_types_end"
